{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Лист1"],"not_rendered":{"charts":1,"images":0,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":79,"n_cols":9,"rows_kept":79,"cut":false,"hidden":false,"merged":[]}
[0,0]
[3.09E-2,39.24]
[6.1800000000000001E-2,166.77]
[9.2700000000000005E-2,156.96]
[0.1236,78.48]
[0.1545,196.20000000000002]
[0.18540000000000001,196.20000000000002]
[0.21629999999999999,176.58]
[0.2472,235.44]
[0.27810000000000001,235.44]
[0.309,235.44]
[0.33989999999999998,235.44]
[0.37080000000000002,235.44]
[0.4017,235.44]
[0.43259999999999998,235.44]
[0.46350000000000002,235.44]
[0.49440000000000001,239.364]
[0.52529999999999999,239.364]
[0.55620000000000003,239.364]
[0.58709999999999996,245.25]
[0.61799999999999999,245.25]
[0.64890000000000003,245.25]
[0.67979999999999996,245.25]
[0.7107,249.17400000000001]
[0.74160000000000004,251.13600000000002]
[0.77249999999999996,251.13600000000002]
[0.8034,251.13600000000002]
[0.83430000000000004,251.13600000000002]
[0.86519999999999997,251.13600000000002]
[0.89610000000000001,255.06]
[0.92700000000000005,255.06]
[0.95789999999999997,255.06]
[0.98880000000000001,255.06]
[1.0197000000000001,255.06]
[1.0506,255.06]
[1.0814999999999999,255.06]
[1.1124000000000001,255.06]
[1.1433,255.06]
[1.1741999999999999,255.06]
[1.2051000000000001,255.06]
[1.236,255.06]
[1.2668999999999999,255.06]
[1.2978000000000001,255.06]
[1.3287,255.06]
[1.3595999999999999,255.06]
[1.3905000000000001,255.06]
[1.4214,255.06]
[1.4522999999999999,255.06]
[1.4832000000000001,255.06]
[1.5141,255.06]
[1.5449999999999999,255.06]
[1.5759000000000001,255.06]
[1.6068,255.06]
[1.6376999999999999,235.44]
[1.6686000000000001,231.51600000000002]
[1.6995,231.51600000000002]
[1.7303999999999999,206.01000000000002]
[1.7613000000000001,176.58]
[1.7922,176.58]
[1.8230999999999999,156.96]
[1.8540000000000001,78.48]
[1.8849,78.48]
[1.9157999999999999,58.86]
[1.9467000000000001,58.86]
[1.9776,39.24]
[2.0085000000000002,39.24]
[2.0394000000000001,0]
[]
[null,null,null,null,null,null," масса топлива / propellant mass"," Mp (kg)",0.46]
[null,null,null,null,null,null," масса заряженного мотора / motor full mass"," Mm (kg)",0.6]
[null,null,null,null,null,null," диаметр мотора / motor diameter"," Dm (m)",0.05]
[null,null,null,null,null,null,"Рассчет / calculated parameters"]
[]
[null,null,null,null,null,null," время работы / trust time"," t (s)",2.0394000000000001]
[null,null,null,null,null,null," макс. тяга / max thrust"," Fmax (N)",254.97289999999998]
[null,null,null,null,null,null," средняя тяга / average thrust"," Favg (N)",211.85335712121221]
[null,null,null,null,null,null," полный импульс / total impulse"," I (N*s)",432.05373651300022]
[null,null,null,null,null,null," удельный импульс / spec. impulse"," Isp (s)",95.776565217391351]
[null,null,null,null,null,null," классификация / classification"," Class","I 212"]